Fuel injection Test Mode

1.	Select ‘Test Mode’ under the ‘Tools’ Menu

2.	Set  test parameters

3.	Burn to ECU

4.	Cycle power – you should come up in Test Mode and the injectors should squirt the specified number of times with the specified pulsewidths and off times. 

5.	Wait until done squirting

6.	When done, go to the Tools/ Test Mode menu. You should still be in Test Mode. Change test parameters if desired, but do NOT burn – you can’t in Test mode. 

7.	If you want to continue/ repeat the test, select ‘Repeat Test’. 

8.	Continue steps 5-7 until you wish to exit test mode or you want to burn the current test parameters. In either case select ‘Normal Mode’.  This will automatically burn the existing test parameters, including the ‘Normal Mode’ selection.

9.	Cycle power and you will be back in ‘Normal Mode’, ready to start the engine or you can repeat from step 1.